### External Device Settings

Use the configuration tool (KV STUDIO/Ver. 2.50) for External Device communication settings. Refer to your External Device manual for details.

1. Start up the configuration tool.

2. From the [File] menu, select [New Project], enter a project name, and then click [OK].

3. In the dialog box that appears, click [Yes] to move to the Unit Editor.

4. Click the [Unit selection (2)] tab, select "KV-LE20A", and then drag and drop the unit between the CPU and the end unit.

5. With KV-LE20A selected, switch to the [Unit setup (3)] tab, and set as follows.

   Setup Items | Settings
   First DM No. | DM10000
   Speed | 100/10 Mbps (automatic)
   IP Address | 192.168.0.1
   Subnet Mask | 255.255.255.0
   Port No. (HOST Link) | 8501

6. From the [File] menu, select [Save and Exit] to return to the editor mode.

7. From the [Monitor/Simulator] menu, select [Convert ➝ Move].

8. Check [Unit setting information], and then click [Exec]. The setting information is transferred.

This completes the setting of the External Device.

NOTE

- Check with your network administrator about the IP address you want to use.
- Do not duplicate IP addresses on the same network.