Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Direct I/O Input | PI00000.0 - PI00223.7 | PIW00000 - PIW00222 |  |
Direct I/O Output | PQ000000.0 - PQ00223.7 | PQW00000 - PQW00222 | *1

*1Write disable

The following devices can only be used for Direct I/O (Packet Transfer).

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
English | German | English | German
Data Block | DB001.DBX00000.0 - DB255.DBX65535.7 | DB001.DBW00000 - DB255.DBW65534 |  |
Input | I00000.0 - I65535.7 | E00000.0 - E65535.7 | IW00000 - IW65534 | EW00000 - EW65534 | *1
Output | Q00000.0 - Q65535.7 | A00000.0 - A65535.7 | QW00000 - QW65534 | AW00000 - AW65534 |
Internal Marker | M00000.0 - M65535.7 | MW00000 - MW65534 |

*1Write disable.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms