### NX1 Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Channel I/O | 0000.00 - 6143.15 | 0000 - 6143 |  |
Internal Auxiliary Relay | W000.00 - W511.15 | W000 - W511 |
Latch Relay | H000.00 - H511.15 | H000 - H511 |
Data Memory | D00000.00 - D32767.15 | D00000 - D32767 |
Extension Data Memory (E0-EC) | E000000.00 - EC32767.15 | E000000 - EC32767 | *1

*1Max 13 bank (E0 to EC) can be used. 1 bank is 32768 words. Available bank number is different depending on the CPU unit.

The device descriptions used in BLUE and the External Device are different. Please be aware of these differences when setting up devices.

Device | BLUE | External Device
--- | --- | ---
Channel I/O | ... | CIO
Internal Auxiliary Relay | W | WR
Latch Relay | H | HR
Data Memory | D | DM
Extension Data Memory (E0-EC) | En | EMn

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms