### Settings of External Device

Use the ladder software (GMWIN) to configure communication settings for the External Device.

Refer to your External Device manual for details.

1. Start up the ladder software.

2. Create the project. Select the using External Device.

3. Select [Basic Parameters] from [Parameter] tab of tree view.

4. Set the setting items as below in the displayed dialog box.

Setup Item | Setting Value
--- | ---
Station number | 0
Baud rate | 38400
Master/Slave | Slave