### 11E)

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block External Device side: Terminal block |
(2) | 2-port adapter II by Pro-face GP070-MD11 |
(3) | Connector conversion cable by Mitsubishi Electric Corp. FX-20P-CADP (0.3m) |
(4) | Function extension board by Mitsubishi Electric Corp. FX1N-422-BD, FX2N-422-BD, FX3U-422-BD or FX3G-422-BD |

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | OFF