### Settings of External Device

NOTE

- When you connect 217IF of which version is "*****_21700_*****" or lower to the Display, set [Wait To Send] to [20ms].

#### Ladder Software Setting

1. Right-click [root] in the browser of the ladder software "CP717" and select [Group Folder] from [New].

NOTE

- Please refer to the manual of the ladder software for the version which supports the Control Pack Series.

2. The [New] dialog box is displayed. Enter the optional group name (ex. "GROUP") and click [OK].

3. The group folder (ex. "GROUP") is created under the [root] in the browser of "CP717". Right-click the folder and select [Order Folder] from [New].

4. The [New] dialog box is displayed. Enter the optional order name (ex. "ORDER") and click [OK].

5. [ORDER] is created under the [root]-[GROUP] in the browser of "CP717". Right-click it and select [PLC Type] from [New].

6. The [PLC Type] dialog box is displayed. Enter the optional PLC name and CPU name and select [CP-9200SH] for [Device Name], then click [OK].

7. The PLC folder (ex. "PLC") is created under the [root]-[GROUP] in the browser of "CP717". The CPU folder (ex. "CPU1") is created under the PLC folder. Double-click [CPU1] to display the [CPU Logon] dialog box.

8. Enter "User name" and "Password" optionally in the [CPU Logon] dialog box and click [OK].

9. Multiple folders are created under the [root]-[GROUP]-[PLC]-[CPU1] in the browser of "CP717". Double-click [Definition Folder]-[Module Configuration] to open the [Engineering Manager] window.

10. Select [CP-9200SH] in [Module] of the [No.00] field in the [Rack1] tab.

11. Select [CP-217] in [Module] of the same [No.] field as your slot number to define the link unit.

12. Double-click the same [No.] as your slot number to display the setting window.

    Setup Items | Setup Description
    --- | ---
    Transmission Protocol | Memobus
    Master/Slave | Slave
    Device address | Device address of the External Device
    Serial I/F | RS-232C
    Transmission Mode | RTU
    Data Length | 8 bits
    Parity Bit | even
    Stop Bit | 1Stop
    Baud Rate | 19.2K
    Send Delay | Not specified

#### Example of Ladder Program

You need the ladder program to connect the Display to the Link I/F CP217IF by YASKAWA Electric Corporation.
The ladder program example is shown below.

NOTE

- This ladder program example enables to communicate the 1 CN port with the Display. Note that each CN port requires the ladder program when you use multiple ports, CN1 to CN3, to communicate simultaneously.
- Use the ladder software to perform the communication settings on the External Device. Those settings are not performed in this ladder program.

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.