### 6B)

No. | Name | Notes
--- | --- | ---
(1) | Mitsubishi PLC FX Series CPU I/F Cable by Pro-face ZC9CBFX11 (1m) or ZC9CBFX51 (5m) |
(2) | Function extension board by Mitsubishi Electric Corp. FX1N-422-BD, FX2N-422-BD, FX3U-422-BD or FX3G-422-BD |

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | ON
4 | OFF