### 1F)

1:1

1:n

n:1

No. | Name | Notes
--- | --- | ---
(1) | MPI Cable (3.5m) by Pro-face CA3-MPI-PGN-PFE or MPI Cable (3.5m) by Pro-face CA3-MPI-PG1-PFE |
(2) | MPI Cable (3.5m) by Pro-face CA3-MPI-PG1-PFE |

IMPORTANT:

- Please turn ON the terminator switch on the connector of the MPI Cable that becomes a terminal on the network.

NOTE

- The cable length have to be 50m or less in one segment.