### 14H

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (plug) External Device side: RJ-45 connector | Instead of connecting the Display (FG), connect the Shield to the Shell.

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- Please turn on the DIP Switch 1 to enable build-in resistance (100Ω) on the remotest External Device side.

- Cable length: 500m or less