### 4H

1:1

1:n

No. | Name | Note
--- | --- | ---
(1) | User-created cable • Connector Display side: D-sub 9 pin (plug) External Device side: Terminal block |

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- The cable length have to be 500m or less. When using FX1N-485-BD, FX2N-485-BD, FX3U-485-BD or FX3G-485-BD, the cable length have to be 50m or less.