Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (Expansion unit) SP5000X (Expansion unit) | 1A | CANopen recommended cable |

IMPORTANT:

- To use the CANopen Slave Driver, you need the CANopen Slave Unit (PFXZCDEUCA1) by Pro-face. Please refer to the CANopen Slave Unit Manual for more details.

NOTE

- Choose a Baud rate that your Bus length can support.

  Baud rate | Bus length
  --- | ---
  1000 Kbps | 20 m
  800 Kbps | 40 m
  500 Kbps | 100 m
  250 Kbps | 250 m
  125 Kbps | 500 m
  50 Kbps | 1000 m

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.