### Setting of External Device

Use the ladder software "PL7-07" for communication settings on External Device.

Select [Programming Port] from [Configuration] in PL7-07 and perform the communication settings as below.

Setup Items | Setup Description
--- | ---
Type | UNI-TELWAY Master
Bit/sec | 19200
DateBits | 8 bits
Parity Odd | Odd
Stop Bits | 1 bit
Number of Slaves | 8

NOTE

- Do not set the address which exceeds "Number of Slaves" on External Device in Server Address and Clients Address. If you set the address which exceeds "Number of Slaves" in Server Address and Clients Address, timeout error will occur, which disables the communication with the External Device. In addition, when you connect many client devices (Display/External Device) on the same serial network, set the longer timeout on the Display.