### 2G

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block Junction side: e-CON connector (plug) |
(2) | Junction by AMP 5-1473574-4 |
(3) | Controller link cable by IAI Corporation CB-RCB-CTL002 |
(4) | Termination resistance Connector Junction side: e-CON connector (plug) |
(5) | User-created cable Connector Junction side: e-CON connector (plug) |

NOTE

- Cable length: 100m or less

*1 The resistance in the Display is used as the termination resistance. Set the value of the DIP Switch on the rear of the Display as shown in the table below.

DIP Switch No. | Set Value
--- | ---
1 | OFF
2 | OFF
3 | OFF
4 | ON