### TCmini series (TC3-01)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External Input Relay | X000 - X00B | X00W - X00W |  | *1
External Output Relay | Y000 - Y00B | Y00W - Y00W | *1
Internal Relay | R000 - R17F | R00W - R17W | *1
Timer Relay | T000 - T05F | T00W - T05W | *1
Counter Relay | C000 - C05F | C00W - C05W | *1
Latch Relay | L000 - L01F | L00W - L01W | *1
Data Register | ------ | D000 - D22F | *1
T/C Register 1 | ------ | P000 - P05F | *1
T/C Register 2 | ------ | V000 - V05F | *1

*1Device format is as follows: Please refer to the manual of External Device for more detail.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms