### External Device Settings

Use the ladder software (GX Works2) by Mitsubishi Electric Corporation for External Device communication settings. Refer to your External Device manual for details.

##### Procedure

1. Start up the ladder software.

2. From the [Project] menu select [New project] to display the [New project] dialog box.

3. Select the series and type of the External Device in use, then click [OK].

4. In the tree view, double-click [PC Parameter] to display the [FX Parameter setting] dialog box.

5. In [FX Parameter setting] click the [Ethernet Port setting] tab, and define the setup items as follows.

   Setup Items | Setting Value
   --- | ---
   CH | CH1
   Input Format | Decimal
   IP address | 192.168.0.1
   Subnet Mask pattern | 255.255.255.0
   Default Router IP Address | 192.168.0.250
   Communication data code | Binary code

6. Click [Open settings], and define the setup items as follows.

   Setup Items | Setting Value
   --- | ---
   Protocol | UDP
   Open system | MC Plotocol (Fixed)
   Host station Port No. (DEC.) | 1025
   Transmission target device IP address (DEC.) | 192.168.0.2
   Transmission target device Port No. (DEC.) | 1025

   NOTE

   - "Transmission target device" refers to the Display.

7. Click [End].

NOTE

- Check with your network administrator about the IP address you want to use.
- Do not duplicate IP addresses on the same network.

NOTE

- To connect FX Series and FX3U-ENET-ADP, you also need Communication adapter or Function extension board.

  CPU | Communication Adapter / Function Extension Board
  FX3S | FX3S-CNV-ADP
  FX3U, FX3UC-32MT-LT(-2) | FX3U-CNV-BD
  FX3UC(D, DS, DSS) | -
  FX3G | FX3G-CNV-ADP

- To connect FX3S, it is necessary to use FX3U-ENET-ADP version 1.20 or later. To connect FX3U/FX3UC/FX3G/FX3GC, it is necessary to use FX3U-ENET-ADP version 1.00 or later.
- Use a FX3U/FX3UC CPU with a system version 3.10 or greater.
- Use a FX3G/FX3GC CPU with a system version 2.00 or greater.