### Settings of External Device

Use the ladder software (MP720 Ver.7.33.0100) to set up communication settings. Set the next contents.

(1) Main CPU settings

(2) Stepping motor settings

For details on communication settings, please refer to the manual of the External Device.

##### Main CPU Settings

1. Start the ladder software.

2. Make a project file. From the [Model] list, select the main CPU.

3. From the [Start] tab, click [Module Configuration].
   [MC-Configurator] starts up.

4. On the CPU you want to use, double-click [218IFD].

5. Click [Parameters] tab.

6. In the [Transmission Parameters] group define the [IP Address] and [Subnet Mask] as follows.

   Setup Items | Setup Description
   --- | ---
   IP Address | 192.168.0.1
   Subnet Mask | 255.255.255.0

7. On the CPU you want to use, set the [SVC32] circuit number to "1".
   Set up the same value as the Display's circuit number.

8. On the CPU you want to use, open [SVC32], and double-click [01 UNDEFINED].

9. In the tree view, from [Stepping], select [Wild Card SteppingMotorDRV], and click [OK].

10. For the [Wild Card SteppingMotorDRV] station number, set "3".

11. Write the settings to the External Device.

IMPORTANT

- To write the settings, select the [Save to flash after transferring to the controller] check box.
  If the data is transferred without selecting the check box, the transferred data is deleted when restarting the External Device.

##### Stepping Motor Settings

Set up communication settings with rotary switches (S1 and S2).

For details on communication settings, please refer to the manual of the External Device.

Rotary Switch | Settings | Setup Description
S1 (x10) | 0 | Station address
S2 (x1) | 3

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.