### PXH series

Device | Bit Address | Word Address | 32bits | Notes
--- | --- | --- | --- | ---
Read Only Word Data | - | 30257 - 31407 |  | *1 *2
Word Data | 40001.00 - 45035.31 | 40001 - 45035 | *2 *3 *4

*1Write disabled.

*2This device is 32 bits in length. Only odd addresses can be assigned.

*3When you write to the bit address, the Display reads the entire word, sets the defined bit, then returns the new word value to the External Device. If the ladder program writes data to this word address during the bit write process, the resulting data may be incorrect.

*4"43153" is an address to order writing in the nonvolatile memory (FIX processing).
Writing in the nonvolatile memory is performed by entering 1 (one) to the writing value.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms