Display (Connection Port) | Cable | Remarks
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*2 | 1A | Connection cable by IAI Corporation CB-ST-E1MW050 |
GP-4115 (COM1) | 1B | User-created cable + Connection cable by IAI Corporation CB-ST-E1MW050 | Cable length: 10m or less.

*2Available only with a COM port that supports RS232C.

IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.