### TOYOPUC-PC3

Device | Bit Address | Byte Address | Word Address | 32bits | Notes
--- | --- | --- | --- | --- | ---
Input Relay | 1X000 - 1X7FF | 1X00L - 1X7FH | 1X00W - 1X7FW |  | *1 *3
2X000 - 2X7FF | 2X00L - 2X7FH | 2X00W - 2X7FW
3X000 - 3X7FF | 3X00L - 3X7FH | 3X00W - 3X7FW
Output Relay | 1Y000 - 1Y7FF | 1Y00L - 1Y7FH | 1Y00W - 1Y7FW | *1 *3
2Y000 - 2Y7FF | 2Y00L - 2Y7FH | 2Y00W - 2Y7FW
3Y000 - 3Y7FF | 3Y00L - 3Y7FH | 3Y00W - 3Y7FW
Internal Relay | 1M000 - 1M7FF | 1M00L - 1M7FH | 1M00W - 1M7FW | *1
2M000 - 2M7FF | 2M00L - 2M7FH | 2M00W - 2M7FW
3M000 - 3M7FF | 3M00L - 3M7FH | 3M00W - 3M7FW
Keep Relay | 1K000 - 1K2FF | 1K00L - 1K2FH | 1K00W - 1K2FW | *1
2K000 - 2K2FF | 2K00L - 2K2FH | 2K00W - 2K2FW
3K000 - 3K2FF | 3K00L - 3K2FH | 3K00W - 3K2FW
Link Relay | 1L000 - 1L7FF | 1L00L - 1L7FH | 1L00W - 1L7FW | *1
2L000 - 2L7FF | 2L00L - 2L7FH | 2L00W - 2L7FW
3L000 - 3L7FF | 3L00L - 3L7FH | 3L00W - 3L7FW
Special Relay | 1V00 - 1VFF | 1V0L - 1VFH | 1V0W - 1VFW | *1
2V00 - 2VFF | 2V0L - 2VFH | 2V0W - 2VFW
3V00 - 3VFF | 3V0L - 3VFH | 3V0W - 3VFW
Timer (Contact) | 1T000 - 1T1FF | 1T00L - 1T1FH | 1T00W - 1T1FW | *1 *3
2T000 - 2T1FF | 2T00L - 2T1FH | 2T00W - 2T1FW
3T000 - 3T1FF | 3T00L - 3T1FH | 3T00W - 3T1FW
Counter (Contact) | 1C000 - 1C1FF | 1C00L - 1C1FH | 1C00W - 1C1FW | *1 *3
2C000 - 2C1FF | 2C00L - 2C1FH | 2C00W - 2C1FW
3C000 - 3C1FF | 3C00L - 3C1FH | 3C00W - 3C1FW
Current Value Register | 1N000-0 - 1N1FF-F | 1N000L - 1N1FFH | 1N000 - 1N1FF | *2
2N000-0 - 2N1FF-F | 2N000L - 2N1FFH | 2N000 - 2N1FF
3N000-0 - 3N1FF-F | 3N000L - 3N1FFH | 3N000 - 3N1FF
Data Register | 1D0000-0 - 1D2FFF-F | 1D0000L - 1D2FFFH | 1D0000 - 1D2FFF | *2
2D0000-0 - 2D2FFF-F | 2D0000L - 2D2FFFH | 2D0000 - 2D2FFF
3D0000-0 - 3D2FFF-F | 3D0000L - 3D2FFFH | 3D0000 - 3D2FFF
Link Register | 1R000-0 - 1R7FF-F | 1R000L - 1R7FFH | 1R000 - 1R7FF | *2
2R000-0 - 2R7FF-F | 2R000L - 2R7FFH | 2R000 - 2R7FF
3R000-0 - 3R7FF-F | 3R000L - 3R7FFH | 3R000 - 3R7FF
Special Register | 1S000-0 - 1S3FF-F | 1S000L - 1S3FFH | 1S000 - 1S3FF | *2
2S000-0 - 2S3FF-F | 2S000L - 2S3FFH | 2S000 - 2S3FF
3S000-0 - 3S3FF-F | 3S000L - 3S3FFH | 3S000 - 3S3FF
File Register | B0000-0 - B1FFF-F | B0000L - B1FFFH | B0000 - B1FFF | *2
Extension Input | EX000 - EX7FF | EX00L - EX7FH | EX00W - EX7FW | *1 *3
Extension Output | EY000 - EY7FF | EY00L - EY7FH | EY00W - EY7FW | *1 *3
Extension Internal Relay | EM0000 - EM1FFF | EM000L - EM1FFH | EM000W - EM1FFW | *1
Extension Special Relay | EV000 - EVFFF | EV00L - EVFFH | EV00W - EVFFW | *1
Extension Keep Relay | EK000 - EKFFF | EK00L - EKFFH | EK00W - EKFFW | *1
Extension Timer | ET000 - ET7FF | ET00L - ET7FH | ET00W - ET7FW | *1 *3
Extension Counter | EC000 - EC7FF | EC00L - EC7FH | EC00W - EC7FW | *1 *3
Extension Link Relay | EL0000 - EL1FFF | EL000L - EL1FFH | EL000W - EL1FFW | *1
Extension 2 Input | GX0000 - GXFFFF | GX000L - GXFFFH | GX000W - GXFFFW | *1 *3
Extension 2 Output | GY0000 - GYFFFF | GY000L - GYFFFH | GY000W - GYFFFW | *1 *3
Extension 2 Internal Relay | GM0000 - GMFFFF | GM000L - GMFFFH | GM000W - GMFFFW | *1
Extension Data Register | U0000-0 - U7FFF-F | U0000L - U7FFFH | U0000 - U7FFF | *2
Extension Setting Value Register | H000-0 - H7FF-F | H000L - H7FFH | H000 - H7FF | *2
Extension Special Register | ES000-0 - ES7FF-F | ES000L - ES7FFH | ES000 - ES7FF | *2
Extension Current Value Register | EN000-0 - EN7FF-F | EN000L - EN7FFH | EN000 - EN7FF | *2
Watch Time Register | ------ | ------ | WT0 - WT6 | *4 *5
Extended Buffer Register | EB00000-0 - EB1FFFF-F | EB00000L - EB1FFFFH | EB00000 - EB1FFFF | *2

*1For word description of the bit device, add "W" to the last of the word address.
Example) When the address is 0 in M device, describe "M0000W".

*2For bit description of the word device, describe "-" following the word address and the bit position next.
Example) When the address is 0 and the bit is 5 in D device, describe " D0000-5".

*3You cannot set the duplicate address for X and Y (EX, EY, GX, GY), T and C (ET, EC).
(Setting such address as X000/Y000, EX000/EY000, T000/C000, ET000/EC000 is wrong.)

*4When you write "Watch Time Register", the Display reads all addresses of "Watch Time Register" in the External Device. Then the Display writes all addresses of "Watch Time Register" after the Display changes the data of your requested address. Note that the correct data may not be written if you change the word address using the ladder program while the Display reads data from the External Device and returns it.

*5Contents of "Watch Time Register" are shown below.

Address | Mean | Note
--- | --- | ---
WT0 | day of week | 0:Sunday, 1:Monday, 2:Tuesday, 3:Wednesday, 4:Thursday, 5:Friday, 6:Saturday
WT1 | year | lower two digits of A.D.
WT2 | month |
WT3 | day |
WT4 | hour | 24-hour system
WT5 | minute |
WT6 | second |

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms