### 3H

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable • Connector Display side: D-sub 9 pin (plug) External Device side: Terminal block | Connect the shield to FG (Shell)

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG's PROFIBUS connector. Do not use it for other devices.

NOTE

- Please set the terminating resistor switch to the "100Ω" position only on the last External Device in the chain.

NOTE

- Total cable length: 500m or less