### H1U/H2U Series

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Register | X000 - X377 | - |  |
Output Relay | Y000 - Y377 | - |
Internal Relay | M0000 - M3071 | - |
Special Relay | M8000 - M8511 | - |
State Relay | S000 - S999 | - |
Timer Contact | T000 - T255 | - |
Timer Register | - | T000 - T255 |
Counter Contact | C000 - C255 | - |
Counter Register | - | C000 - C199 |
- | C200 - C255 | *1
Data Register | - | D0000 - D8255 |

*132-bit device

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms