### Settings of External Device

Communication setting of communication module CPU unit by ladder software. (Check the operation in MPE720 Ver.6)

##### Ladder Software Setting

1. Start ladder software, make an order folder and a PLC folder in a root folder.
   Select the connected PLC at the time of PLC folder making.

2. Click the right button of the PLC which select logon in the displayed menu.

   NOTE

   - Logon after confirming that a check does not begin [online] of a displayed menu.
   - Refer to User's Manual of the PLC about a method of logon.

3. Double-click the [Definition folder]-[Module constitution] of the PLC folder, and display [Engineering Manager].

4. Select the rack classification and link I/F, the pull-down menu in [Controller] of [Engineerring Manager].
   Set the number corresponding to the slot number that a communication module uses.
   Select the communication module, setting contents are displayed to [Module details] of [Enginnering Manager].

5. Double-click the number part at No. in [Module details].
   Double-click the slot number connecting the ethernet unit.

6. Select [Transmission Parameters] tab, and set the setup items as follows.

   Setup Items | Setup Description
   --- | ---
   IP Address | 192.168.0.1
   Subnet Mask | 255.255.255.0

7. Click [Easy Setting] in [Transmission Parameters] tab to display [Message Communication Easy Setting] dialog box.

8. Set the setup items as follows, and click [OK].

   Setup Items | Setup Description
   --- | ---
   Connection No. | 1
   MP Series Port No. | 1024
   Communication protocol Type | Extended MEMOBUS
   Connect Type | UDP
   Code | BIN
   Node Port IP Address*1 | 192.168.0.10
   Other Device Port No.*1 | 1024

*1Set the IP address and the port number of the Display.

9. Double-click [Setting] to display [Automatically Reception Setting] dialog box.

10. Select "Enable" of [Automatically Reception], and click [OK].

11. Turn the DIP switch "INIT" of a communication module to ON, and supply the power.

12. Forward communication setting and a ladder program to a communication module.

13. Log on the PLC in online and write the transferred data to the flash memory.

14. Turn the PLC power and the INIT DIP switch to OFF. Then, turn the PLC power to ON.

#####

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.
- Please refer to the manual of the ladder software for more detail.
- When Automatically Reception is disabled for messages, the ladder program for communication is required.

##### Ladder Program for Communication