### H / EH-150 / MICRO-EH Series

Device | Bit Address | Word Address | Double Word Address | 32 bit | Remarks
--- | --- | --- | --- | --- | ---
External Input | X00000-X05A95 | WX0000-WX05A7 | DX0000-DX05A6 |  | *1 *2
External Output | Y00000-Y05A95 | WY0000-WY05A7 | DY0000-DY05A6 | *2
Remote Input Relay | X10000-X49995 | WX1000-WX4997 | DX1000-DX4996 | *1 *3
Remote Output Relay | Y10000-Y49995 | WY1000-WY4997 | DY1000-DY4996 | *3
Inner Output | R000-R7BF | - | - |
Special Inner Output | R7C0-R7FF | - | - |
Data Area | M0000-M3FFF | WM000-WM3FF | DM000-DM3FE |
First CPU Link | L00000-L03FFF | WL0000-WL03FF | DL0000-DL03FE |
Second CPU Link | L10000-L13FFF | WL1000-WL13FF | DL1000-DL13FE |
On Delay Timer | TD000 -TD255 | - | - |
Single-shot Timer | SS000-SS255 | - | - |
Watchdog Timer | WDT000-WDT255 | - | - |
Mono Stable Timer | MS000-MS255 | - | - |
Retentive Timer | TMR000-TMR255 | - | - |
Up Counter | CU000-CU511 | - | - |
Ring Counter | RCU000-RCU511 | - | - |
Up-down Counter | CT000-CT511 | - | - |
Timer Counter (Elapsed Value) | - | TC000-TC511 | - |
Word Inner Output | - | WR0000-WRC3FF | DR0000-DRC3FE |
Network Link Area | - | WN0000-WN7FFF | DN0000-DN7FFE |

*1Write disable *2Specify as shown below. (Example) External input unit No.1, Slot No.2, Inner Module Bit No.34 (Example) External input unit No.1, Slot No.2, Inner Module Word No.3 *3Specify as shown below. (Example) Remote External Input Remote Master No.1, Remote Slave No.2, Slot No.3, Inner Module Bit No.45 (Example) Remote External Input Remote Master No.1, Remote Slave No.2, Slot No.3, Inner Module Word No.4

NOTE

- Available type and range of device vary depending on CPU. Be sure to check them in each CPU manual before using.

#### CPU How to set address when using the link

Set the check box of "Use CPU Link" to ON.

When using CPU Link, loop No. and unit No. are added to the address.

(Example) Loop No.1, Unit No.2

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms