Display (Connection Port) | Cable | Remarks
--- | --- | ---
SP5000 (Expansion Unit) SP5000X (Expansion Unit) | 1A | Type A cable for PROFIBUS-DP |

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.

IMPORTANT:

- To use the PROFIBUS DP Slave Driver, you need the PROFIBUS DP Slave/MPI Unit (PFXZCDEUPF1) by Pro-face. Please refer to the PROFIBUS DP Slave/MPI Unit Manual for more details.

NOTE

- Choose a Baud rate that your Bus length can support.

- Baud rate | Bus length
  --- | ---
  12 Mbps | 100 m
  6 Mbps
  3 Mbps
  1.5 Mbps | 200 m
  500 Kbps | 400 m
  187.5 Kbps | 1000 m
  93.75 Kbps | 1200 m
  19.2 Kbps
  9.6 Kbps