### Settings of External Device

Communication setting of External Device by ladder software (TCPRGOS-W (J)).

Please refer to the manual of the External Device for more details.

##### Procedure

1. Start the ladder software of the computer.

2. Select [Register editor] in the [Tool] menu.
   [Register data [online]] window is displayed.

3. Click [A].

4. Double click the special auxiliary relay (A00F, A154, A155) to set communication speed.

   Communication speed | A00F | A154 | A155
   --- | --- | --- | ---
   9600bps | OFF | OFF | OFF

NOTE

- The other settings of communication speed is as follows.

Communication speed | A00F | A154 | A155
--- | --- | --- | ---
19200bps | ON | OFF | OFF
38400bps | *1 | ON | OFF
57600bps | OFF | ON
115200bps | ON | ON

*1Either ON or OFF can be set.

NOTE

- To connect the Display directly to the External Device, in BLUE open the halo menu and set PC No. to 64.