Display (Connection Port) | Cable | Notes
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 1A | COM port Conversion Adapter by Pro-face CA3-ADPCOM-01 + Terminal block Conversion Adapter by Pro-face CA3-ADPTRM-01 + User-created cable | Cable length: 15m or less.
1B | User-created cable
1G | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable
GP-4116 (COM1) | 1E | User-created cable | Cable length: 15m or less.
PS5000 PS6000 (Optional Interface) PSA6000 *7 | 1I | User-created cable | Cable length: 15m or less.

*b-3Except ST-6200

*7Only the COM port which can communicate by RS-422/485 (2 wire) can be used.

IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.