### 4F)

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 |
(2) | User-created cable Connector Display side: Terminal block External Device side: Terminal block | Connect the shield to FG (Shell).

NOTE

- Cable length: 500m or less.

- Turn on the DIP Switch for Terminating Resistance Settings on the External Device located at the end.