Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 10E | User-created cable + Mitsubishi PLC A, QnA, FX Series 2 Port Adapter II by Pro-face GP070-MD11 + Connector conversion cable by Mitsubishi Electric Corp.*4 FX-20P-CADP (0.3m) | Cable length: 600m or less.
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*c-2 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 10F | 2-port adapter cable by Pro-face PFXZCBCBMD1 + Mitsubishi PLC A, QnA, FX Series 2 Port Adapter II by Pro-face GP070-MD11 + Connector conversion cable by Mitsubishi Electric Corp.*4 FX-20P-CADP (0.3m) | Cable length: 600m or less.
10A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + 2-port adapter cable for AGP by Pro-face CA3-MDCB11 (5m) + Mitsubishi PLC A, QnA, FX Series 2 Port Adapter II by Pro-face GP070-MD11 + Connector conversion cable by Mitsubishi Electric Corp.*4 FX-20P-CADP (0.3m)
10B | User-created cable + Mitsubishi PLC A, QnA, FX Series 2 Port Adapter II by Pro-face GP070-MD11 + Connector conversion cable by Mitsubishi Electric Corp.*4 FX-20P-CADP (0.3m)
PS5000 PS6000 (Optional Interface) PSA6000 *8 | 10G | User-created cable + Mitsubishi PLC A, QnA, FX Series 2 Port Adapter II by Pro-face GP070-MD11 + Connector conversion cable by Mitsubishi Electric Corp.*4 FX-20P-CADP (0.3m) | Cable length: 600m or less.

*4For FX2, the connector conversion cable (FX-20P-CADP) by Mitsubishi Electric Corp. is not necessary.

*c-2Except ST-6200

*8Only the COM port which can communicate by RS-422/485 (4 wire) can be used.

IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.