#### CJ2 Series

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
Channel I/O | 0000.00 - 6143.15 | 0000 - 6143 |  | *1
Internal Auxiliary Relay | W000.00 - W511.15 | W000 - W511 |
Special Auxiliary Relay | A0000.00 - A1471.15 A10000.00 - A11535.15 | A0000 - A1471 A10000 - A11535 | *2
Latch Relay | H000.00 - H511.15 | H000 - H511 |
Timer (Time Up Flag) | T0000 - T4095 | - | *3
Counter (Count Up Flag) | C0000 - C4095 | - | *3
Timer (Current Value) | - | T0000 - T4095 |
Counter (Current Value) | - | C0000 - C4095 |
Data Memory | D00000.00 - D32767.15 | D00000 - D32767 | *1
Extension Data Memory (E0-E18) | E0 00000.00 - E18 32767.15 | E0 00000 - E18 32767 | *4
Extension Data Memory (Current Bank) | - | EM00000 - EM32767 |
Task Flag (Bit) | TKB000 - TKB127 | - | *3
Task Flag (Status) | TK000.00 - TK127.07 | TK000 - TK126 | *3
Index Register | - | IR00 - IR15 | *5
Data Register | - | DR00 - DR15 | *5

*1Do not write in Channel I/O address 1500-1899 and Data Memory address D30000-D31599 from the Display. Because those address are used for setting the system on the External Device.

*2Write disable in A000 - A447 and A10000 - A11535.

*3Write disable

*4Max 24 bank (E0 to E18) can be used. 1 bank is 32768 words. Available bank number is different depending on the CPU unit.

*5Write disable during RUN

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms