### Settings of External Device

Use the ladder software "RSLogix 5" for communication settings.

Open "Channel Configuration" of "RSLogix 5" to perform the settings in the "Chan. 0" tab.

##### For Full Duplex

Setup Items | Setup Description
--- | ---
Communication Mode | System (Point-To-Point)
Baud Rate | 19200
Parity | NONE
Bits per Char | 8
Stop Bits | 1
Control Line | No Handshaking
Error Detection | CRC
Embedded Responses | Auto-detect
Detect Duplicate Messages | Disabled
ACK Timeout | 50
NAK Receive | 3
DF1 ENQs | 3
MSG Application Timeout | 30 seconds
Station Address | 0

##### For Half Duplex

Setup Items | Setup Description
--- | ---
Communication Mode | System (Slave)
Baud Rate | 19200
Parity | NONE
Bits per Char | 8
Stop Bits | 1
Control Line | No Handshaking
Error Detection | CRC
Detect Duplicate Messages | Disabled
RTS Send Delay | 0
RTS Off Delay | 0
ACK Timeout | 50
DF1 Retries | 3
MSG Application Timeout | 30 seconds
Station Address | 0

NOTE

- Please refer to the manual of the ladder software for more detail on other setting description.