### Setting of External Device

##### When using the multi communication unit AFP2465 combined with the communication block AFP2804 or AFP2805

Set the station setting switch to [1] and set the transmission format setting switch as below.

DIP Switch | Settings | Setup Description
SW1 | ON | Operation mode on the COM1 Computer link
SW2 | ON
SW3 | ON | Transmission speed on the COM1 19200bps
SW4 | OFF
SW5 | ON | Operation mode on the COM2 Computer link
SW6 | ON
SW7 | ON | Transmission speed on the COM2 19200bps
SW8 | OFF

NOTE

- AFP2465 is the multi communication unit of FP2/FP2SH.
  AFP2084 and AFP2085 are the communication blocks attached to AFP2465.