### Control Pack (CP-9200/CP-9200H)

Device | Bit Address | Register No of CP-9200/CP-9200H (equivalent to the address) | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Register | 00001-02048 | IB00000-IB007FF |  | *1 *2
Output Register | 02049-04096 | OB00000-OB007FF | *1 *2
System Register | 10001-12048 | SB000000-SB00127F (S Register of CPU#0) | *1 *2 *3

Device | Word Address | Register No of CP-9200/CP-9200H (equivalent to the address) | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Register | 49744-49871 | IB00000-IB007FF |  |
Output Register | 49872-49999 | OB00000-OB007FF |
System Register | 30001-30256 | SW00000-SW00255 (S Register of CPU#0) | *3
Data Register | 31001-33048 (CP-9200H only) | DW00000-DW02047 (D Register of CPU#1) | *3
40001-42048 | DW00000-DW02047 (D Register of CPU#0) |
Common Register | 42049-49743 | MW00000-MW07694 |

*1 When you write the bit address, the Display reads the word address corresponding to that of the External Device first. Then, it changes the target bit address among the word data once read and returns the word data to the External Device. Note that the correct data may not be read if you change the word address value in the ladder program while the Display reads the data of the External Device and returns it to the External Device.

*2 Specification using the word address is also available.

*3 Write disable

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms