Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Data | 04096,00 -36678,15 | 04096 - 36678 |  | *1

*1When bits are written, the Display reads the corresponding word address from the External Device, sets particular bits of that word address to ON, and then returns the resulting address to the External Device. Note that the correct data may not be written if you change the word address using the ladder program while the Display reads data from the External Device and returns it.

IMPORTANT:

- Refer to your External Device manual for precautions on device reading and writing.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms
- Even if you use a nonexistent address, the read error may not be displayed. In this case, "0" is retained for the read data. Note that the write error is displayed.