### CS1 Series

Device | Bit Address | Word Address | 32 bit | Remarks
--- | --- | --- | --- | ---
Channel IO Area | 0000.00-6143.15 | 0000-6143 |  | *1
Internal Auxiliary Relay | W000.00-W511.15 | W000-W511 |
Special Auxiliary Relay | A00000.00-A00959.15 | A00000-A00959 | *2
Hold Relay | H0000.00-H0511.15 | H0000-H0511 |
Timer (Completion Flag) | T0000-T4095 | - | *3
Counter (Completion Flag) | C0000-C4095 | - | *3
Timer (Preset Value) | - | T0000-T4095 |
Counter (Preset Value) | - | C0000-C4095 |
Data Memory | D00000.00-D32767.15 | D00000-D32767 | *1
EM Area (E0-EC) | E000000.00-EC32767.15 | E000000-EC32767 | *4
EM Area (Current bank) | EM00000.00-EM32767.15 | EM00000-EM32767 |
Task Flag Area (Bit) | TKB000-TKB031 | - | *3
Task Flag Area (Status) | TK000.00-TK031.07 | TK000-TK030 | *3
Index Registers | - | IR00-IR15 | *5
Data Registers | - | DR00-DR15 | *5

*1Data memory addresses D30000-D31599 and Channel IO Area addresses 1500-1899 are used as the area for system settings on the External Device side; do not write data from the Display. Refer to your External Device manual for details.

*2Cannot write to A000-A447.

*3Write disabled

*4Up to 13 banks (E0-EC) can be used. One bank is 32768 words. The number of banks differs depending on the CPU unit.

*5Cannot write while in RUN mode.

NOTE

- When using the CS1 series, set the [String Encode] to Shift JIS under the BLUE System Configuration.
- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms