### Settings of External Device

Use the programming panel for communication settings of the External Device.

Please refer to the manual of the External Device for more details.

#### Procedure

1. Perform the following communication settings in the programming panel.

   Setup Items | Setup Description
   --- | ---
   Address | 1
   Baud Rate | 9600
   Parity Setting | Enable
   Parity Type | Even
   Stop Bit Length | 1
   Data Bit Length | 8 (RTU mode)
   Port Delay Timer | 10 ms