### Settings of External Device

Use the LS ELECTRIC setting tool (XG-PD Editor) to configure communication settings for the External Device.

Refer to your External Device manual for details.

1. Start up the setting tool.

2. Select base and slot which using module is connected from [Standard settings] tab in offline, and [Communication Module Settings] dialog box is displayed.

3. Select "Cnet" from [Type], and click [OK].

4. Select [Connect] from [Online] menu.

5. Select [Read IO Information] from the [Online] menu.

6. Double click [Cnet] from the [Standard settings] tab, and [Standard Settings-Cnet] dialog box is displayed.

7. Set [Channel 1] setup items as follows, and click [OK].

   Setup Item | Setting Value
   --- | ---
   Type | RS485
   Speed | 38400
   Data Bit | 8
   Stop Bit | 1
   Parity Bit | NONE
   Modem Type | Null Modem
   Station | 0
   Active mode | XGT server

8. Select [Write Parameter] from the [Online] menu, and [Write Parameter] dialog box is displayed.

9. Select using module, and click [OK].

10. Select [Reset] from the [Online] menu.