Display (Connection Port) | Cable*1 | Remarks
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000 (COM1) STM6000 (COM1) PC/AT IPC*3 | 1A | By Hitachi IES Co., Ltd. WVCB02H | Cable length: 15m or less
1B | User-created cable1
1C | User-created cable2
GP-4115 (COM1) | 1D | User-created cable1 | Cable length: 15m or less
1E | User-created cable2

*1You need to change the wiring depending on the speed.

| H-200 H-250 H-252B | H-252C | H-300/H-302 H-700/H-702 H-2000/H-2002 | H-4010
--- | --- | --- | --- | ---
Speed | Wiring | Speed | Wiring | Speed | Wiring | Speed | Wiring
Peripheral Port 1 | 2400bps 4800bps 9600bps | 1B, 1D | 2400bps 4800bps 9600bps 19200bps | 1A, 1B, 1C, 1D, 1E | 4800bps | 1B, 1D | 4800bps | 1B, 1D
19200bps | 1A, 1C, 1E | 19200bps | 1A, 1C, 1E | 19200bps | 1A, 1C, 1E
38400bps | 1A, 1B, 1C, 1D, 1E
Peripheral Port 2 | - | - | 4800bps | 1B, 1D | - | - | 4800bps | 1B, 1D
19200bps | 1A, 1C, 1E | 19200bps | 1A, 1C, 1E
38400bps | 1A, 1B, 1C, 1D, 1E

*3Only the COM port which can communicate by RS-232C can be used.

IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.