### External Device Settings

Use Connected Components Workbench for communication setting.

Please refer to the manual of Connected Components Workbench for more information.

1. Connect the PC and External Device with an Ethernet cable.

2. Start Connected Components Workbench.

3. From the menu bar, select [File]-[New…], and create a new project.

4. In the Add Device window, select the appropriate controller.

5. Click [Select]-[Add To Project].

6. In the project tree view select [Micro850], and in the Micro850 tree view select [Ethernet].

7. In the Internet Protocol (IP) Settings, select [Configure IP address and settings], and set the following properties.

Setup Items | Setting Value
--- | ---
IP Address | 192.168.1.1
Subnet Mask | 255.255.255.0

NOTE

- When selecting "Micro 800 Series Native", you need to create a Tag Data Block.
  "Micro800 Series Native"

- Check with a network administrator about IP address. Do not set the duplicate IP address.

- Set IP address on the External Device for IP address in Device-specific settings.

- You need to set IP address on the Display in the offline mode of the Display.

- To use the tags set in Connected Components Workbench, you need to import a CSV file. Even if you enter the tag name in the device address setting, it may not work properly.