### Setting of External Device

Communication setting of External Device using setting tool (PC Interface Software for RC) of External Device.

Please refer to the manual of the External Device for more details.

##### Procedure

1. Start up the setting tool.

2. Select [Teach mode1 (Safety speed effective/PIO start prohibition)] of a window to select manual operation mode.

3. Select [Controller Setup]-[Assign Axis Number] from [Setting] menu.

4. Set axis number of [Assign Axis Number] dialog box as follows, and click [OK].

   Setup Item | Setting Value
   --- | ---
   New Assign Axis Number | 0

5. Expand the axis number to be set from the tree view and click [Parameter].

6. Set [SIO Baudrate[bps]] of External Device as follows.

   Setup Item | Setting Value
   --- | ---
   SIO Baudrate[bps] | 38400

7. Select [Send to Controller] from the [Parameter] menu and send the set contents to the controller.