### 1H)

1:1

n:1

No. | Name | Note
--- | --- | ---
(1) | User-created cable Connector Display side: D-Sub 9 pin (plug) External Device side: Depends on the specification of the External Device. | Instead of connecting the Display (FG), connect the Shield to the Shell.

IMPORTANT:

- The 5V output (Pin #6) on the Display is the power for the Siemens AG’s PROFIBUS connector. Do not use it for other devices.

NOTE

- Cable length: 1,000m or less (Depends on master's capacity).