Display (Connection Port) | Cable | Notes
--- | --- | ---
GP-4116 (COM1) | 7E | User-created cable | Total cable length: 500m or less
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*c-2 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 7F | RS-422 Terminal Block Conversion Adapter by Pro-face PFXZCBADTM1 + User-created cable | Total cable length: 500m or less
7A | COM port conversion adapter by Pro-face CA3-ADPCOM-01 + Terminal block conversion adapter by Pro-face CA3-ADPTRM-01 + User-created cable
7B | User-created cable
PS5000 PS6000 (Optional Interface) PSA6000 *2 | 7G | User-created cable | Total cable length: 500m or less

*c-2Except ST-6200 *2Only the COM port which can communicate by RS-422/485 (4 wire) can be used. IPC COM Port

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.