### 7J

1:1

1:n

No. | Name | Notes
--- | --- | ---
(1) | User-created cable Connector Display side: Terminal block RS232C conversion unit side: D-Sub 9 pin (plug) |
(2) | RS232C conversion unit by IAI Corporation RCB-CV-MW |
(3) | Communication cable by IAI Corporation CB-RCA-SIO050 |
(4) | SIO converter by IAI Corporation RC*-TU-SIO-* |
(5) | User-created cable Connector SIO converter side (TB1): Link connection terminal block Insulated PIO side (TB2): Terminal block |
(6) | Insulated PIO terminal block by IAI Corporation RC*-TU-PIO-* |
(7) | Power & I/O Cable by IAI Corporation CB-ERC-PWBIO***-H6 or CB-ERC-PWBIO***-RB-H6 |

NOTE

- Set the termination resistance connection switch of the PIO terminal block on the end to RTON side.
- Cable length from SIO converter to External Device: 100m or less

*1 We recommend the IAI Corporation CB-ERC-PWBIO***-H6 or CB-ERC-PWBIO***-RB-H6 as the Power & I/O Cable.