### TCmini series (TC8-00/TC5-02)

Device | Bit Address | Word Address | 32 bits | Notes
--- | --- | --- | --- | ---
External Input Relay | Photo coupler | X000 - X00F | X00W - X00W |  | *1
DIP Switch | X010 - X017 | X01W - X01W | *1
Extended Panel Switch | X100 - X11F | X10W - X11W | *1
External Output Relay | Transistor | Y020 - Y02B | Y02W - Y02W | *1
Relay Contact | Y02C - Y02F | Y02W - Y02W | *1
Extended Panel LED | Y140 - Y14F | Y14W - Y14W | *1
Internal Relay | R000 - R77F | R00W - R77W | *1
Edge Relay | E000 - E17F | E00W - E17W | *1
Latch Relay | L000 - L07F | L00W - L07W | *1
Timer Relay | T000 - T27F | T00W - T27W | *1
Counter Relay | C000 - C27F | C00W - C27W | *1
Special AUX Relay | A000 - A16F | A00W - A16W | *1
Data Register | ------ | D000 - D77F | *1
T/C Register 1 | ------ | P000 - P27F | *1
T/C Register 2 | ------ | V000 - V27F | *1

*1Device format is as follows: Please refer to the manual of External Device for more detail.

NOTE

- Please refer to the precautions on manual notation for icons in the table
  Supported Devices Symbol and Terms