### External Device Settings

Use the PU/EXT key, MODE key, M dial and SET key in the operation panel of the CPU unit for External Device communication settings.

Refer to your External Device manual for details.

1. Turn ON the power supply.

2. Press PU/EXT key to select the PU operation mode.

3. Press MODE key to select the parameter setting mode.

4. Display the setting parameter number with M dial.

5. Press SET key to display the current setting value.

6. Set the setting value with M dial.

7. Press SET key to confirm the setting value.

Setting Parameter Number | Setting Value | Setup Description
--- | --- | ---
117 | 0 | PU communication station number
118 | 192 | PU communication speed
119 | 1 | PU communication stop bit length
120 | 2 | PU communication parity check
121 | 1 | Number of PU communication retries
122 | Any Except 0 | PU communication check time interval
123 | 9999 | PU communication waiting time setting
124 | 1 | PU communication CR/LF presence/absence selection

NOTE

- Always restart the External Device after changing parameters.