### KV-Nano Series

Device | Bit Address | Word Address | 32 bits | Remarks
--- | --- | --- | --- | ---
Input Relay | R00000 - R59915 | R000 - R599 |  |
Output Relay |
Internal Auxiliary Relay |
Link Relay | B0000 - B1FFF | B000 - B1FF | *5
Internal Auxiliary Relay | MR00000 - MR59915 | MR000 - MR599 |
Latch Relay | LR00000 - LR19915 | LR000 - LR199 |
Control Relay | CR0000 - CR8915 | CR00 - CR89 |
Work Relay | VB0000 - VB1FFF | VB000 - VB1FF | *5
Timer (Contact) | T0000 - T0511 | ----- | - |
Counter (Contact) | C0000 - C0255 | ----- |
High-speed Counter Comparator (Contact) | CTC0 - CTC7 | ----- | *1 *4
Timer (Setting Value) | ----- | TS0000 - TS0511 |  | *2
Counter (Setting Value) | ----- | CS0000 - CS0255 | *2
Timer (Current Value) | ----- | TC0000 - TC0511 | *2
Counter (Current Value) | ----- | CC0000 - CC0255 | *2
Data Memory | ----- | DM00000 - DM32767 |
Temporary Data Memory | ----- | TM000 - TM511 |
Control Memory | ----- | CM00000 - CM08999 |
Link Register | ----- | W0000 - W3FFF |
Work Memory | ----- | VM00000 - VM09499 |
Index Register | ----- | Z01 - Z12 | *2 *3
High-speed Counter (Current Value) | ----- | CTH0 - CTH3 | *2 *4
High-speed Counter Comparator (Setting Value) | ----- | CTC0 - CTC7 | *2 *4

*1Write disable

*232-bit device

*3Z11 and Z12, used by the External Device system, are not available to write in.

*4If KV-NC32T access the device which is out of range, an error does not occur. The value will be zero (0).

*5The word address descriptions used in the BLUE and the External Device are different. Please be aware of these differences when setting up word addresses.

BLUE | External Device
B000 - B1FF | B0000 - B1FF0
VB000 - VB1FF | VB0000 - VB1FF0

NOTE

- Please refer to the precautions on manual notation for icons in the table.

Supported Devices Symbol and Terms