### External Device Settings

For External Device communication settings, use the ladder software (Si-Wave V2.08).

Refer to your External Device manual for details.

1. Start up the ladder software.

2. Open [Parameter] window.

3. Select parameter to set.

4. Input setting value as shown below in each parameter.

   Parameter No. | Setting Value | Setup Description
   --- | --- | ---
   00 | 0 | Axis Number
   43 | 0 | COM. Format

5. Click [Write in to Servo].

Communication settings are complete.