### Settings of External Device

For details on communication settings, please refer to the manual of the External Device.

##### Setup Procedure

1. Press UP to display the Parameter Setting Mode screen. Press ENTER to change to Set Up Mode.

2. Press UP to display setup items. Press ENTER key to change to setup screen.

3. Press UP or RESET to select the setup value. Press ENTER to set up a description.

##### Setup Description

Setup Items | Setup value | Description
--- | --- | ---
b1-02*1 | 3 | Run Command Selection (Option Card)
F6-20 | 21 | MECHATROLINK station address
F6-22 | 0 | MECHATROLINK link rate (10Mbps)

*1Set b1-01 to 3 when you set the frequency via MECHATROLINK.