### PLC-5 Series

Device | Bit Address | Word Address | 32 bit | Remarks
--- | --- | --- | --- | ---
Input File | I:000/00-I:377/17 | I:000-I:377 |  | *2
Output File | O:000/00-O:377/17 | O:000-O:377 | *2
Status File | S:000/00-S:163/15 | S:000-S:163 |
Bit File | B003:000/00-B999:999/15 | B003:000-B999:999 |
Timer File | Enable | T003:000/-T999:999/ | EN | T003:000.-T999:999. | - |
Timing | TT | -
Done | DN | -
Preset | - | PRE
Accumu-lated | - | ACC
Counter File | Up Enable | C003:000/-C999:999/ | CU | C003:000.-C999:999. | - |
Down Enable | CD | -
Done | DN | -
Overflow | OV | -
Underflow | UN | -
Update Acc. | UA | -
Preset | - | PRE
Accumu-lated | - | ACC
Control File | Enable | R003:000/-R999:999/ | EN | R003:000.-R999:999. | - |  |
Enable Unload | EU | -
Done | DN | -
Empty | EM | -
Error | ER | -
Unload | UL | -
Inhibit Comp. | IN | -
Found | FD | -
Length | - | LEN
Position | - | POS
Integer File | - | N003:000-N999:999 |
Floating Point File | - | F003:000-F999:999 | - | 32 Bit Access Only
String File | - | ST003:000-ST999:999 |  | *1
ASCII File | - | A003:000-A999:999 |
BCD File | - | D003:000-D999:999 |

*1The maximum length of the String File device is 82 bytes.

*2Input (I) and Output (O) element addresses are defined using Octal data format. Valid word address ranges are: 0-7, 10-17, 20-27, ... 360-367, 370-377. Valid bit address ranges are: 0/0-0/7 and 0/10-0/17, 1/0-1/7 and 1/10-1/17, ... 377/0-377/7 and 377/10-377/17.

NOTE

- Please refer to the precautions on manual notation for icons in the table.
  Supported Devices Symbol and Terms