Display (Connection Port) | Cable | Remarks
--- | --- | ---
SP5000 (COM1/2) SP5000X (COM1/2) ST6000*b-3 (COM2) ST-6200 (COM1) STM6000 (COM1) PS6000 Basic Box (COM1/2) | 10A | User created cable | Cable length: 1000m or less.
GP-4116 (COM1) | 10B | User created cable | Cable length: 1000m or less.
PS5000 PS6000 (Optional Interface) PSA6000 *8 | 10C | User created cable | Cable length: 1000m or less.

*b-3Except ST-6200

*8Only the COM port which can communicate by RS-422/485 (2 wire) can be used.

IPC COM Port

IMPORTANT:

- The RS-422/485 cable length is normally 1000m or less, which depends on the External Device. Please refer to the manual of the External Device for more details.
- The connection method and termination resistance depends on the External Device.
- The termination resistance on the Display is not isolated.

DANGER

ELECTRIC SHOCK

Ensure that the ground connection for each component of interconnected equipment is reliably connected to the same ground potential (within 100 ohms) prior to connecting the equipment.

WARNING

UNINTENDED EQUIPMENT OPERATION

- Use shielded twisted-pair cables.

- Connect the cable shields, then connect the cable to a single-point ground on the Display side.