### External Device Settings

Use the configuration software (ConfiguratorWD) to set up communication settings on the External Device.

For details on communication settings, please refer to the manual of the External Device.

1. Start up the configuration software.

2. From the [Option] menu, select [Select the IP of PC] to display the [Setting IP Address] window.

3. Select the [Specify the IP address of PC] option, and click [OK].

4. From the [Search] menu, select the [Search BroadCast] option.
   The connected External Device will appear.

5. Click the External Device to set up its IP address, and from the [Edit] menu select the [Setting IP Address] command.

6. Select the [Use this IP Address] option.

7. Set the IP Address to "192.168.1.5", and click [OK].

8. From the [Edit] menu, select [Communication Setting] to display the [Communication Setting] window.

9. Set the items to the following values, and click [OK].

   Setup Item | Setting description
   --- | ---
   Protocol Mode | UDP
   Action Mode | Server Mode
   Communication Mode | MEWTOCOL
   Source Port No. | 60001
   Timeout | 15

10. Click [OK].

NOTE

- Check with a network administrator about IP address. Do not set the duplicate IP address.